高德地图SDK(导航) V11.2.0501

Loading...
Searching...
No Matches
Properties | List of all members
AMapNaviIntervalCameraDynamicInfo Class Reference

`#include <AMapNaviCommonObj.h>`

Inheritance diagram for AMapNaviIntervalCameraDynamicInfo:

## Properties
NSInteger | length
NSInteger | remainDistance
NSInteger | averageSpeed
NSInteger | reasonableSpeedInRemainDist

## Detailed Description

区间测速电子眼的动态信息 since 6.0.0 Dynamic information of the section speed camera

## Property Documentation

## ◆ averageSpeed

- (NSInteger) averageSpeed
| read write nonatomic assign

进入区间测速路段后的实时平均车速 The real-time average speed after entering the section speed section

## ◆ length

- (NSInteger) length
| read write nonatomic assign

区间测速路段的总长度 The total length of the section speed section

## ◆ reasonableSpeedInRemainDist

- (NSInteger) reasonableSpeedInRemainDist
| read write nonatomic assign

进入区间测速路段后的剩余路段的合理车速 Reasonable speed for the remaining section after entering the interval speed measurement section

## ◆ remainDistance

- (NSInteger) remainDistance
| read write nonatomic assign

进入区间测速路段后实时的区间路段剩余长度 The remaining length of the section speed section in real time after entering the section speed section

The documentation for this class was generated from the following file:

- AMapNaviCommonObj.h

© 2017 高德信息技术有限公司 版权所有，保留所有权利。